Early War Aircraft Characteristics Chart

AlliedAircraft Stability Engine Wings Fuselage Tail Fuel Armament Max. Alt. Avro 504K A 6 32 28 5 60 1FL VH Bristol Scout D B 6 20 21 5 45 1FL # H+ DeHaviland DH-2 B 6 25 25 6 45 1FL H Morane-Saulnier N / L C 6 16 22 4 45 1F H Nieuport 11 B 6 19 19 4 45 1FL VH Nieuport 12 B 6 24 23 4 45 1OL VH Nieuport 17 B 6 13 20 4 45 1F* VH RAF RE-8 B 8 40 27 6 52 1F, 1OL H+ Sopwith 1 1/2 Strutter A 6 28 25 6 60 1F, 1OL H+ Sopwith Pup B 6 19 25 4 50 1F VH Spad VII B 8 22 20 5 52 1F VH Vickers F.B.5 ’Gun Bus’ B 6 36 27 6 60 1FL M+

German Aircraft Stability Engine Wings Fuselage Tail Fuel Armament Max. Alt. Albatros D-I / D-II B 8 24 24 6 49 2F VH Fokker E-III C 6 17 23 4 45 1F H Halberstadt D-II B 8 25 24 4 45 1F VH Pfalz E-III C 6 16 22 4 45 1F H Roland C-II B 8 30 25 6 65 1F, 1O H Siemens-Schuckert D-I B 6 13 20 4 45 1F VH + - Aircraft my regain maximum altitude # - Bristol also flew unarmed and with single Vickers (1F) * - Some Nieuport 17s flew with additional 1FL

Early War Designer’s Notes

Band Altitude Range Speed # MPH @ G.L. VL 0 - 4K 1 Below 91 L 4K - 8K 2 91 - 100 M 8K - 12K 3 101 - 110 H 12K - 16K 4 115 and above VH 17K and up